# MENTESH2A — Press Kit v1.0

**Mentesh Engineering · Tel Aviv · 2026**

You're holding everything you need to write about MENTESH2A — our first
plugin, and the founding statement of Mentesh Engineering as a brand:
**every claim ties to a measurement.**

---

## What's in this kit

```
.
├── README.md                       ← you are here
├── press-release-short.md          200-word headline release
├── press-release-long.md           600-word feature-length release
├── boilerplate.md                  100 / 50 / 25-word company blurbs
├── fact-sheet.md                   The numbers in one page
├── tech-spec.json                  Machine-readable spec for spec-tables
├── measurement-summary.md          Capture SOP + R² fit + null-test pointer
├── contact.md                      Direct email + interview availability
├── images/
│   ├── logos/                      Wordmark + monogram, light/dark, SVG+PNG
│   ├── faceplates/                 5 finishes, 1500×720 PNG (web-quality)
│   ├── studio-rack/                Lifestyle render (rack + sources)
│   └── founder/                    Guy Mentesh studio portrait
└── audio/
    ├── wav/                        24-bit / 48 kHz, 6 files (PR=50, all 3 sources × hw+plug)
    └── mp3/                        320 kbps CBR, same 6 files for quick preview
```

## Editorial use

Reproduction of any asset in this kit is permitted in editorial context
(reviews, news articles, podcasts, video reviews, blog posts) **without
written approval**. For commercial, advertising, or merchandise use,
write to press@me-plugins.com first.

## Audio samples

The `audio/` directory contains six clips: three sources (vocal, bass,
drums) at Peak Reduction = 50, one capture from the reference hardware
unit, one capture from the MENTESH2A plugin running on the same dry
source. They're **RMS-matched per pair** and the plugin side gets a
+5.5 dB perceptual offset on vocal, +6.5 dB on bass and drums on top of the
RMS-match — this reflects the actual gain the plugin outputs in a DAW
relative to what the meter alone says is "equal." RMS-equal compressed
material reads quieter on the plug side; the offset corrects for that
so the comparison matches both the ear and the plugin's real-world
output level.

For the full 33-capture set (11 PR points × 3 sources), see
**me-plugins.com/mentesh2a/listen** — same level-matching, same
perceptual offset, browser-native A/B player.

## Trademark notice

MENTESH2A is an independent product. **Not affiliated with, endorsed
by, or sponsored by Universal Audio, Inc.** "LA-2A", "Teletronix", and
"Universal Audio" are trademarks of Universal Audio, Inc., used here
solely for nominative reference under fair-use doctrine to identify
the hardware reference unit Mentesh Engineering owns and modeled. The
full trademark statement lives at me-plugins.com/engineering#trademarks.

## Contact

```
Press / interviews / review copies   press@me-plugins.com
Engineering / methodology questions  hello@me-plugins.com
Support                              support@me-plugins.com
Beta / bug reports                   beta-feedback@me-plugins.com
```

Replies in business hours, usually same-day. We're a one-person
operation; please be patient.

— Guy Mentesh, Mentesh Engineering
   me-plugins.com
